# Assignment 4

|  |  |
| --- | --- |
| Date | 3 Nov 2022 |
| Name | C.V.Gowsikha |
| Team ID | PNT2022TMID40586 |
| Project Name | Project-IoT Based Industry Specific Intelligent Fire Management System |

**Write code and connections in wokwi for ultrasonic sensor. Whenever distance is less than 100 cms send alert to ibm cloud and display in device recent events. Upload document with wokwi share link and images of ibmcloud**

# Code

#include <WiFi.h> #include

<PubSubClient.h>WiFiClient wifiClient; String data3; #define ORG "ozyf7e"

#define DEVICE\_TYPE "AnuESP" #define DEVICE\_ID "Anu123" #define TOKEN "12345678"

#define speed 0.034

#define led 14

char server[] = ORG ".messaging.internetofthings.ibmcloud.com";char publishTopic[]

= "iot-2/evt/shreedharen/fmt/json";

char topic[] = "iot-2/cmd/led/fmt/String";char authMethod[] = "use-token-auth";

char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;

PubSubClient client(server, 1883, wifiClient); const int trigpin=5; const int echopin=18;String

command; String data=""; long duration;float

dist; void setup()

{

**Serial**.begin(115200); pinMode(led, OUTPUT);

pinMode(trigpin, OUTPUT); pinMode(echopin, INPUT); wifiConnect(); mqttConnect();

}

void loop() {

bool isNearby = dist < 100; digitalWrite(led, isNearby); publishData();

delay(500);

if (!client.loop()) { mqttConnect();

}

}

void wifiConnect() {

**Serial**.print("Connecting to "); **Serial**.print("Wifi"); WiFi.begin("Wokwi-GUEST", "", 6);

while (WiFi.status() != WL\_CONNECTED) { delay(500);

**Serial**.print(".");

}

**Serial**.print("WiFi connected, IP address: ");

**Serial**.println(WiFi.localIP());

}

void mqttConnect() {

if (!client.connected()) {

**Serial**.print("Reconnecting MQTT client to ");

**Serial**.println(server);

while (!client.connect(clientId, authMethod, token)) {

**Serial**.print("."); delay(500);

}

initManagedDevice();

**Serial**.println();

}

}

void initManagedDevice() { if (client.subscribe(topic)) {

// Serial.println(client.subscribe(topic));

**Serial**.println("IBM subscribe to cmd OK");

} else {

**Serial**.println("subscribe to cmd FAILED");

}

}

void publishData()

{

digitalWrite(trigpin,LOW); digitalWrite(trigpin,HIGH); delayMicroseconds(10); digitalWrite(trigpin,LOW); duration=pulseIn(echopin,HIGH); dist=duration\*speed/2; if(dist<100){

String payload = "{\"Alert Distance\":";payload += dist;

payload += "}"; **Serial**.print("\n"); **Serial**.print("Sending payload: "); **Serial**.println(payload);

if (client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish OK");

}

}

if(dist>100){

String payload = "{\"Distance\":";payload += dist;

payload += "}"; **Serial**.print("\n"); **Serial**.print("Sending payload: "); **Serial**.println(payload);

if(client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish OK");

}else {


**Serial**.println("Publish FAILED");

}


}

}

**Connections**



**Output:**



**Cloud image:**

